Millview-Updated Site Map

* Install a concrete border along the edge of the asphalt (approximately 927 feet). Concrete 12” wide x 6” depth. Control joints every ~~12 feet~~. Top of border to be set at existing asphalt grade.
* Control joints every 10 feet.

West Courts

* Six-foot square around south end tree 12” wide x 6” depth. Top of border to be set at existing asphalt grade.
* Remove the sidewalk leading from the parking lot gate to basketball courts. Replace with new concrete. Approximately ~~15’x5’x4”~~ 18’x5’x4” and 7’x10.5’x4”
* No Approach
* No Asphalt

Fire Lane and NE Courts

* Remove 12-inch wide section of asphalt approximately 637 feet in length. Replace with concrete 12” wide x 6” depth. Control joints every ~~12 feet.~~ Top of border to be set at existing asphalt grade.
* Control joints every 10 feet.

